**Statement of product composition**

|  |  |
| --- | --- |
| **Purpose:** | 1. To ensure the integrity of waterproofing products are not compromised, and that products meet certification requirements. 2. This form, to be completed by an APAS signatory, is used when submitting a product for APAS certification against a nominated specification. 3. Retain a copy as a record. |
| **Instructions:** | 1. Use one application form per product. 2. Fill in the form by completing the sections, as applicable. 3. Ensure that the product name appearing on this documentation (and the PDS/TDS, & SDS) is the same as that which appears on the product label as it is this name and/or number that will be listed on the [APAS List of Certified Products](https://vs.csiro.au/apas/list-of-certified-products/). |

|  |  |
| --- | --- |
| SECTION A: Background information | |
| Manufacturer: (including name, RMU No.(s) & location(s) where manufacture occurs) | Click to enter manufacturer details |
| Product code: | Click to enter product code |
| Product name: | Click to enter product name |
| Parent product revision no.: (data describing this product derived from design revision no.) | Click to enter revision no. |
| APAS specification no.: (including sub-class, if applicable) | Click to enter APAS specification no. |
| APAS ID (for resubmissions and/or Parent Products only) | Click to enter APAS ID |

|  |  |
| --- | --- |
| SECTION B: Composition of the product  NOTE:   * Refer to the relevant [APAS specification](https://vs.csiro.au/apas/specifications/) for information pertaining to product composition, testing specifications etc; * State the waterproof product type (SM, DPC of F) and its compositional materials. The following are typical (but are not limited to) materials for each type: * Sheet Membranes (SM): PVC, bituminous, pliable/non-pliable board, felt, laminated aluminium foil. * Damp Proof Course (DPC): metal, bitumen coated metal, polyethylene coated metal, bitumen impregnated without material without a metal centre or polyethylene. * Flashing (F): aluminium, steel, zinc, or copper. | |
| Waterproof product type | **Compositional material(s)** |
| Click to enter product type | Click to enter compositional material |
| Click to enter product type | Click to enter compositional material |
| Click to enter product type | Click to enter compositional material |
| Click to enter product type | Click to enter compositional material |

|  |  |
| --- | --- |
| SECTION C: Packaging properties  NOTE:   * Example of packaging properties (examples only; please state actual product packaging properties): * Sheet Membranes (SM): Sheet – 3m x 1m, purchased individually or in packs of 50 sheets. * Damp Proof Course (DPC): Roll – 30cm x 15m, purchased individually or in packs of 6. * Flashing (F): Continuous length cut to size and set lengths of 5m, 10m or 20m. | |
| Waterproof product type | **Physical attributes** |
| Click to enter product type | Click to enter physical attributes |
| Click to enter product type | Click to enter physical attributes |
| Click to enter product type | Click to enter physical attributes |
| Click to enter product type | Click to enter physical attributes |

|  |  |  |
| --- | --- | --- |
| SECTION D: QC Parameters | | |
| Waterproof product type | **QC testing performed1** | **Standard &/or specification associated with the QC test2** |
| Click to enter product type | Click to enter QC test | Click to enter standard/spec |
| Click to enter product type | Click to enter QC test | Click to enter standard/spec |
| Click to enter product type | Click to enter QC test | Click to enter standard/spec |
| Click to enter product type | Click to enter QC test | Click to enter standard/spec |
| Click to enter product type | Click to enter QC test | Click to enter standard/spec |
| Click to enter product type | Click to enter QC test | Click to enter standard/spec |

1 Batch to batch QC testing that is routinely undertaken.  
2 Specification &/or standard can be AS/NZS, ASTM, ISO, in-house variations of test methods etc.,

|  |  |
| --- | --- |
| SECTION E: Declaration  NOTE: To be completed by an APAS signatory of the RMU. | |
| I hereby declare that (check each box): | |
| This information conforms with all the requirements of clause 5 of APAS document AP-D192, and | |
| The information provided is true and correct to the best of my knowledge. | |
| APAS signatory name: | Click to enter APAS signatory name |
| Signature (not required if submitted electronically): |  |
| Date: | Click to enter a date |

|  |  |
| --- | --- |
| FOR APAS USE ONLY: | |
| Determination: (Approved/Not Approved) |  |
| Approval Class: (CLASS I or CLASS II) |  |
| If not approved, state reason(s): |  |
| Name of APAS Personnel: |  |
| Signature: (not required if submitted electronically) |  |
| Date: |  |
| APAS ID: (for new approvals) |  |